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AC-Photo-initiated cure. A curing process in cured-in-place pipe (CIPP) rehabilitation where a resin liner is exposed to light of a specific wavelength, which activates chemical polymerization that ultimately transforms liquid resin into a solid structural pipe within the original host pipe.

AC-PLUMBER (MASTER). The term “Master Plumber” shall mean a person other than a 
journeyman or apprentice plumber, who is not on inactive status, having satisfied the 
Allegheny County Health Department as to his knowledge of the installation of plumbing 
and has been licensed by the Department to install plumbing as a Master Plumber.

PLUMBING. The practice, materials and fixtures utilized in the installation, maintenance, 
extension and alteration of all piping, fixtures, plumbing appliances and plumbing 
appurtenances, within or adjacent to any structure, in connection with sanitary drainage or 
storm drainage facilities; venting systems; and public or private water supply systems.

PLUMBING APPLIANCE. Any one of a special class of plumbing fixtures intended to 
perform a special function. Included are fixtures having the operation or control dependent 
on one or more energized components, such as motors, controls, heating elements, or 
pressure- or temperature-sensing elements.

Such fixtures are manually adjusted or controlled by the owner or operator, or are operated 
automatically through one or more of the following actions: a time cycle, a temperature 
range, a pressure range, a measured volume or weight

Chapter 7 Sanitary Drainage
717.7 Installation. The installation of relining materials shall be performed in accordance 
with the manufacturer's installation instructions, applicable referenced standards and this 
code.

717.7.1 Material data report. The installer shall record the data as required by the relining 
material manufacturer and applicable standards. The recorded data shall include but is not 
limited to the location of the project, relining material type, amount of product installed 
and conditions of the installation. A copy of the data report shall be provided to the code 
official prior to final approval.

717.8 Post-installation recorded video camera survey. The completed, relined piping 
system shall be inspected internally by a recorded video camera survey after the system 
has been flushed and flow-tested with water. The video survey shall be submitted to the 
code official prior to finalization of the permit. The video survey shall be reviewed and 
evaluated to provide verification that no defects exist. Any defects identified shall be 
repaired and replaced in accordance with this code.

717.9 Certification. A certification shall be provided in writing to the code official, from the 
permit holder, that the relining materials have been installed in accordance with the 
manufacturer's installation instructions, the applicable standards and this code.

717.10 Approval. Upon verification of compliance with the requirements of Sections 717.1  through 717.9, the code official shall approve the installation.

SECTION 718
REHABILITATION OF BUILDING SEWERS AND BUILDING DRAINS INSIGHTS
AC-718.1 Cure-in-place. Sectional cure-in-place rehabilitation of building sewer 
piping and sewer service lateral piping shall be in accordance with ASTM F2599.
Photo-initiated curing shall be used for the rehabilitation of building 
sewer piping by cured-in-place pipe (CIPP) methods and in accordance with ASTM F1216, ASTM F1743, ASTM F3541, or ASTM F2599. Main and lateral cure-in-place rehabilitation of building sewer and sewer service lateral pipe and their connections to the main sewer pipe shall be in accordance with ASTM F2561. Hydrophilic rings or gaskets in cure-in-place rehabilitation of building sewer piping and sewer service laterals shall be in accordance with ASTM F3240 to ensure water tightness and elimination of ground water penetration
